Through-hole package

1N914 & 1N4148 in DO-35 glass axial package.      [image: C:\Users\Tony\Documents\Lazer\Internet Parts\914.png]         


Surface-mount packages

[image: C:\Users\Tony\Documents\Lazer\Internet Parts\914-SMD.jpg]			LL914 & LL4148 in MiniMELF package. 
		                                              
1N4148W in SOD-123 package.                                 [image: ]
Note: Some 1N4148 family surface-mount packages are marked with "T4" text.

Specifications

Absolute maximum ratings (stress ratings, consult datasheet for recommended ratings).
VRRM = 100 V  (maximum repetitive reverse voltage)
IO = 200 mA  (average rectified forward current)
IF = 300 mA  (DC forward current)
If = 400 mA  (recurring peak forward current)
IFSM = 1 A at 1 s pulse width; 4 A at 1 μs pulse width (non-repetitive peak forward surge current)

Electrical and Thermal characteristics:
VF = 1 V at 10 mA (maximum forward voltage) 

VR = 75 V at 5 μA; 100 V at 100 μA (minimum breakdown voltage and reverse leakage current)

trr = 4 ns (maximum reverse-recovery time)

[bookmark: _GoBack]PD = 500 mW (maximum power dissipation
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Typical 1n914 Diode Electrical Symbol
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